|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Treatment** | **Polymer tested** | **Origin/Supplier** | **State of samples** | **Condition of the water in the tank** |
| • Pristine  • Artificially dry weathered  • Artificially seawater weathered  • Artificially biofouled on pristine surface  • Artificially biofouled on rough surface  • Field | • PS  • PE  • PP  • PET amorphous  • PET crystalline  • PVC  • Extruded polystyrene  •Thermoplastic elastomer  • Fluorocarbon  • Paraffin  •PA6 | • Carat  • The Ocean Cleanup  • Shop  • Port of Antwerp  • Scheldt  • VITO  • Marine Remote Sensing Group | • Dry  • Wet  • Submerged | • Clear water, no turbidity  • Algae:  1.Nominal conc. 3000 cells/ml  2.Nominal conc. 1500 cells/ml  • Sediment:  1.SSC 4mg/L  2.SSC 16mg/L |

add 'PA6'